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Plasterer safety checklist
Trade-specific safety checks for plasterers - run through before work starts, every time.
Site address: ________________________________________________________________________________
Date: ________________________________________________________________________________
Checked by: ________________________________________________________________________________
Checks
[ ] Dust - mask worn when mixing plaster; background ventilated   Yes [ ]   No [ ]   N/A [ ]
[ ] Manual handling - 25kg bags lifted correctly; mixer positioned safely   Yes [ ]   No [ ]   N/A [ ]
[ ] Working at height - hop-ups and platforms stable for ceiling work   Yes [ ]   No [ ]   N/A [ ]
[ ] Slips - wet plaster spills cleaned; sheeting secured   Yes [ ]   No [ ]   N/A [ ]
[ ] Eye protection - worn when mixing and when working overhead   Yes [ ]   No [ ]   N/A [ ]
[ ] Skin - gloves or barrier cream; wash hands before eating   Yes [ ]   No [ ]   N/A [ ]
[ ] Electrical safety - sockets masked, not painted over; power off if needed   Yes [ ]   No [ ]   N/A [ ]
[ ] PPE worn - dust mask, eye protection, gloves as a minimum   Yes [ ]   No [ ]   N/A [ ]
[ ] Site left safe - tools cleaned, buckets emptied, area swept   Yes [ ]   No [ ]   N/A [ ]
[ ] Drying - customer advised on drying times before decorating   Yes [ ]   No [ ]   N/A [ ]
Actions required [List any issues found and what was done]
Sign-off
Checked by: ____________________   Signature: ____________________   Date: ____________________
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