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Tiler safety checklist
Trade-specific safety checks for tilers - run through before work starts, every time.
Site address: ________________________________________________________________________________
Date: ________________________________________________________________________________
Checked by: ________________________________________________________________________________
Checks
[ ] Dust - mask worn when cutting tiles; wet cutting preferred  Yes [ ]  No [ ]  N/A [ ]
[ ] Manual handling - tile boxes lifted with bent knees; no overloading  Yes [ ]  No [ ]  N/A [ ]
[ ] Slips - wet floors signed and dried; spills cleaned immediately  Yes [ ]  No [ ]  N/A [ ]
[ ] Eye protection - worn when cutting, drilling or mixing  Yes [ ]  No [ ]  N/A [ ]
[ ] Knee protection - knee pads for floor work  Yes [ ]  No [ ]  N/A [ ]
[ ] Electrical safety - power isolated where tiling near sockets or showers  Yes [ ]  No [ ]  N/A [ ]
[ ] Sharp edges - cut tiles handled with gloves  Yes [ ]  No [ ]  N/A [ ]
[ ] Ventilation - adequate airflow when using solvent-based adhesives  Yes [ ]  No [ ]  N/A [ ]
[ ] PPE worn - eye protection, dust mask, knee pads, gloves as needed  Yes [ ]  No [ ]  N/A [ ]
[ ] Site left safe - offcuts cleared, tools secured, area clean  Yes [ ]  No [ ]  N/A [ ]
Actions required [List any issues found and what was done]
Sign-off
Checked by: ____________________   Signature: ____________________   Date: ____________________
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